GSIC - Global Service Information Center

# SPEEDOMETER DRIVEN GEAR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE VEHICLE SPEED SENSOR WITH SPEEDOMETER DRIVEN GEAR SUB-ASSEMBLY

1. Disconnect the sensor connector.

1. Remove the bolt and sensor with the driven gear.

3. REMOVE SPEEDOMETER DRIVEN GEAR SUB-ASSEMBLY

1. Remove the clip and driven gear from the sensor.

1. Remove the O-ring from the driven gear.