GSIC - Global Service Information Center

### REAR PLANETARY GEAR > DISASSEMBLY

1. REMOVE OUTPUT SHAFT

2. REMOVE PLANETARY OUTPUT SHAFT OIL SEAL RING

3. REMOVE REAR PLANETARY RING GEAR

4. INSPECT NO. 2 ONE-WAY CLUTCH

5. REMOVE NO. 2 ONE-WAY CLUTCH

6. REMOVE NO. 2 PLANETARY CARRIER THRUST WASHER

7. REMOVE NO. 1 PLANETARY CARRIER THRUST WASHER

8. REMOVE REAR PLANETARY FLANGE THRUST NEEDLE ROLLER BEARING

9. REMOVE REAR PLANETARY RING GEAR FLANGE

10. INSPECT PLANETARY PINION GEAR THRUST CLEARANCE