GSIC - Global Service Information Center

# CRANKSHAFT POSITION SENSOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE NO. 1 ENGINE UNDER COVER

3. REMOVE NO. 2 ENGINE UNDER COVER

4. REMOVE CRANKSHAFT POSITION SENSOR

1. Disconnect the sensor connector.

1. Remove the 3 clips, bolt and sensor.