GSIC - Global Service Information Center

# CLUTCH RELEASE CYLINDER (except 1GR-FE) > INSTALLATION

## for Preparation Click here

1. INSTALL CLUTCH RELEASE CYLINDER ASSEMBLY

1. Install the clutch release cylinder with the 2 bolts.

   Torque:
     12 N*m{ 122 kgf*cm , 9 ft.*lbf }

2. CONNECT CLUTCH RELEASE CYLINDER FLEXIBLE TUBE

1. Using SST, connect the flexible tube.

   SST
     09023-00101

   Torque:
     15 N*m{ 153 kgf*cm , 11 ft.*lbf } for use without SST
     14 N*m{ 143 kgf*cm , 10 ft.*lbf } for use with SST

   HINT:
     Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

3. BLEED AIR FROM CLUTCH PIPE LINE

1. Fill the master cylinder reservoir with fluid.

   Torque:
     11 N*m{ 112 kgf*cm , 8 ft.*lbf }

1. Bleed air from the clutch system.

4. CHECK FOR CLUTCH FLUID LEAKAGE

1. Check for clutch fluid leakage (Click here).

5. CHECK FLUID LEVEL IN RESERVOIR

1. Check fluid level in reservoir (Click here).