GSIC - Global Service Information Center

### DTC P0351 Ignition Coil "A" Primary / Secondary Circuit

DESCRIPTION

WIRING DIAGRAM

INSPECTION PROCEDURE

CHECK SPARK PLUG AND SPARK OF MISFIRING CYLINDER

CHECK WIRE HARNESS (IGNITION COIL ASSEMBLY - ECM (IGF SIGNAL TERMINAL))

INSPECT ECM (IGF1 VOLTAGE)

CHECK WIRE HARNESS (IGNITION COIL ASSEMBLY - ECM (IGT SIGNAL TERMINAL))

INSPECT ECM (IGT1, IGT2, IGT3, IGT4, IGT5 OR IGT6 VOLTAGE)

INSPECT ECM (IGT1, IGT2, IGT3, IGT4, IGT5 OR IGT6 VOLTAGE)

INSPECT IGNITION COIL ASSEMBLY (POWER SOURCE)

CHECK WIRE HARNESS (IGNITION COIL ASSEMBLY - IGNITION SWITCH)