GSIC - Global Service Information Center

# SFI SYSTEM > PRECAUTION

## for Preparation Click here

NOTICE:

  Perform the RESET MEMORY (A/T initialization) operation after replacing the automatic transmission assembly, engine assembly or ECM.

  A750E: Refer to the Initialization (Click here).

  A750F: Refer to the Initialization (Click here).

System Name | See procedure
Combination meter | Click here

HINT:

  RESET MEMORY cannot be completed by only disconnecting the cable from the negative (-) battery terminal.