GSIC - Global Service Information Center

# COUNTER GEAR AND REVERSE IDLER GEAR > INSTALLATION

## for Preparation Click here

1. INSTALL COUNTER GEAR FRONT BEARING

1. Using SST and a press, press in the front bearing to the counter gear.

   SST
     09515-10010

   NOTICE:
     Install it so that the snap ring groove of the bearing faces to the front side.

2. INSTALL NO. 2 COUNTER GEAR FRONT BEARING SNAP RING

1. Select a snap ring that makes the clearance between the counter gear and snap ring to be within the specification.

   Standard clearance:
     0.1 mm (0.0039 in.) or less

     Mark | Thickness
     A | 2.05 to 2.10 mm (0.0807 to 0.0827 in.)
     B | 2.10 to 2.15 mm (0.0827 to 0.0846 in.)
     C | 2.15 to 2.20 mm (0.0846 to 0.0866 in.)
     D | 2.20 to 2.25 mm (0.0866 to 0.0886 in.)
     E | 2.25 to 2.30 mm (0.0886 to 0.0906 in.)
     F | 2.30 to 2.35 mm (0.0906 to 0.0925 in.)

1. Using a snap ring expander, install the snap ring.