GSIC - Global Service Information Center

# TRANSMITTER BATTERY > REMOVAL

1. REMOVE TRANSMITTER HOUSING COVER

NOTICE:

  Take extra care when handling these precision electronic components.

1. Twist the screwdriver in the direction of the arrow mark in the illustration, and open the transmitter housing cover.

   NOTICE:
     Do not forcibly pry the cover.

   HINT:
     Tape the screwdriver tip before use.

2. REMOVE DOOR CONTROL TRANSMITTER MODULE

1. Remove the door control transmitter module.

3. REMOVE TRANSMITTER BATTERY

1. Detach the hook of the transmitter battery's cover and remove the cover.

1. Remove the battery (lithium battery).

   NOTICE:
   1. Do not push the terminals with your finger.
   2. Do not forcibly pry up the battery (lithium battery: CR2016). The terminals may become damaged.
   3. Do not touch the battery with wet hands. Water may cause rust.
   4. Do not touch or move any components inside the transmitter. It may cease to work.