GSIC - Global Service Information Center

# CLUTCH RELEASE CYLINDER (for 1GR-FE) > REMOVAL

## for Preparation Click here

1. DRAIN CLUTCH FLUID

2. REMOVE RELEASE CYLINDER HEAT INSULATOR

1. Remove the bolt, nut and insulator.

3. DISCONNECT CLUTCH RELEASE CYLINDER FLEXIBLE TUBE

1. Using SST, remove the flexible tube.

   SST
     09023-00101

   HINT:
     Use a container to catch the fluid.

1. Using SST, disconnect the flexible tube.

   SST
     09023-00101

   HINT:
     Use a container to catch the fluid.

1. Remove the bolt and 2 way.

4. REMOVE CLUTCH RELEASE CYLINDER ASSEMBLY

1. Remove the 2 bolts and clutch release cylinder.