GSIC - Global Service Information Center

# FRONT BUMPER > DISASSEMBLY

## for Preparation Click here

1. REMOVE NO. 1 RADIATOR GRILLE RETAINER

1. Remove the 5 screws and retainer.

2. REMOVE RADIATOR GRILLE NAME PLATE (for 1GR-FE)

1. Remove the 2 spring nuts.

1. Using a heat light, heat the name plate.

   Standard:

     Item | Heating Temperature
     Name Plate | 20 to 30°C (68 to 86°F)

   NOTICE:
     Do not heat the name plate excessively.

1. Pull off the name plate by cutting the double-sided tape with a knife.

   NOTICE:
     Be careful not to damage the radiator grille.

3. REMOVE RADIATOR GRILLE EMBLEM

1. Using a screwdriver, detach the 3 claws and remove the emblem from the radiator grille.

4. REMOVE FRONT BUMPER EXTENSION LH (w/ Front Bumper Extension)

1. Using a screwdriver, detach the 6 clips and remove the extension.

   HINT:
     Tape the screwdriver tip before use.

5. REMOVE FRONT BUMPER EXTENSION RH (w/ Front Bumper Extension)

HINT:

  Use the same procedures described for the LH side.

6. REMOVE FRONT BUMPER HOLE COVER LH

1. Using a screwdriver, remove the clip and hole cover.

   HINT:
     Tape the screwdriver tip before use.

7. REMOVE FRONT BUMPER HOLE COVER RH

HINT:

  Use the same procedures described for the LH side.

8. REMOVE NO. 2 FRONT BUMPER EXTENSION INSERT LH

1. Remove the screw and extension insert.

9. REMOVE NO. 2 FRONT BUMPER EXTENSION INSERT RH

1. Remove the screw and extension insert.