GSIC - Global Service Information Center

# THERMOSTAT > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. DRAIN ENGINE COOLANT

1. Remove the radiator cap.

1. Loosen the cylinder block drain cock plug and radiator drain plug, and then drain the coolant.

   HINT:
     Collect the coolant in a container and dispose of it according to the regulations in your area.

3. DISCONNECT RADIATOR HOSE OUTLET

4. REMOVE WATER INLET

1. Remove the power steering pump's connector.

1. Remove the 2 nuts, bolt and inlet.

5. REMOVE THERMOSTAT