GSIC - Global Service Information Center

### THERMOSTAT > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. DRAIN ENGINE COOLANT

4. REMOVE AIR CLEANER ASSEMBLY

5. REMOVE NO. 1 ENGINE COVER SUB-ASSEMBLY

6. REMOVE CHARGE AIR COOLER ASSEMBLY

7. REMOVE COMPRESSOR INLET ELBOW

8. DISCONNECT RADIATOR HOSE INLET

9. REMOVE NO. 1 AUTOMATIC TRANSMISSION OIL COOLER TUBE CLAMP (for Automatic Transmission)

10. REMOVE WATER INLET

11. REMOVE THERMOSTAT