GSIC - Global Service Information Center

# TRANSMISSION WIRE > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. DRAIN AUTOMATIC TRANSMISSION FLUID

1. Remove the drain plug and gasket, and drain ATF.

1. Install a new gasket and the drain plug.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

3. REMOVE AUTOMATIC TRANSMISSION OIL PAN SUB-ASSEMBLY

NOTICE:

  Some fluid will remain in the oil pan.

1. Remove the 20 bolts.

1. Examine the particles in the pan.

   1. Remove the magnets and use them to collect steel particles. Carefully inspect the foreign matter and particles in the pan and on the magnets to anticipate the type of wear you will find in the transmission.
      Steel (magnetic): bearing, gear and clutch plate wear
      Brass (non-magnetic): bushing wear

4. REMOVE VALVE BODY OIL STRAINER ASSEMBLY

1. Remove the 4 bolts and oil strainer.

   NOTICE:
     Be careful as some fluid will come out of the oil strainer.

5. SEPARATE TRANSMISSION WIRE

1. Remove the 2 bolts and clamp.

1. Disconnect the ATF temperature sensor.

1. Disconnect the 7 connectors from the solenoid valves.

6. REMOVE TRANSMISSION WIRE

1. Disconnect the transmission wire connector.

1. Remove the bolt and pull out the transmission wire.