GSIC - Global Service Information Center

# AIR FUEL RATIO SENSOR (for Sensor 1) > INSTALLATION

## for Preparation Click here

1. INSTALL AIR FUEL RATIO SENSOR (for Bank 1 Sensor 1)

1. Using SST, install the sensor to the exhaust manifold.

   SST
     09224-00010

   Torque:
     40 N*m{ 408 kgf*cm , 30 ft.*lbf } for use with SST
     44 N*m{ 449 kgf*cm , 32 ft.*lbf } for use without SST

   HINT:
     Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

1. Connect the sensor connector.

2. INSTALL AIR FUEL RATIO SENSOR (for Bank 2 Sensor 1)

SST
  09224-00010

1. Using SST, install the sensor to the exhaust manifold.

   Torque:
     40 N*m{ 408 kgf*cm , 30 ft.*lbf } for use with SST
     44 N*m{ 449 kgf*cm , 32 ft.*lbf } for use without SST
   Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

1. Connect the sensor connector.

3. INSTALL V-BANK COVER

1. Install the cover with the 2 nuts.

   Torque:
     7.5 N*m{ 76.5 kgf*cm , 66 in.*lbf }

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.