GSIC - Global Service Information Center

### WATER PUMP > REMOVAL

1. DISCONNECT NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. DRAIN ENGINE COOLANT

4. REMOVE V-BANK COVER

5. DISCONNECT RADIATOR HOSE INLET

6. DISCONNECT RADIATOR HOSE OUTLET

7. REMOVE FAN SHROUD

8. DISCONNECT NO. 2 VENTILATION HOSE

9. REMOVE AIR CLEANER ASSEMBLY

10. REMOVE WATER INLET HOUSING

11. REMOVE NO. 2 IDLER PULLEY SUB-ASSEMBLY

12. REMOVE GENERATOR ASSEMBLY

13. REMOVE V-RIBBED BELT TENSIONER ASSEMBLY

14. REMOVE WATER PUMP ASSEMBLY