GSIC - Global Service Information Center

### THERMOSTAT > INSTALLATION

1. INSTALL THERMOSTAT

2. INSTALL WATER INLET

3. INSTALL NO. 1 AUTOMATIC TRANSMISSION OIL COOLER TUBE CLAMP (for Automatic Transmission)

4. INSTALL COMPRESSOR INLET ELBOW

5. CONNECT RADIATOR HOSE INLET

6. INSTALL CHARGE AIR COOLER ASSEMBLY

7. INSTALL NO. 1 ENGINE COVER SUB-ASSEMBLY

8. INSTALL AIR CLEANER ASSEMBLY

9. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

10. ADD ENGINE COOLANT

11. CHECK FOR ENGINE COOLANT LEAKS

12. INSTALL NO. 1 ENGINE UNDER COVER

13. PERFORM INITIALIZATION