GSIC - Global Service Information Center

### STEERING COLUMN ASSEMBLY > REMOVAL

1. PRECAUTION

2. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

3. PLACE FRONT WHEELS FACING STRAIGHT AHEAD

4. REMOVE STEERING PAD ASSEMBLY

5. REMOVE STEERING WHEEL ASSEMBLY

6. REMOVE STEERING COLUMN LOWER COVER

7. REMOVE STEERING COLUMN UPPER COVER

8. REMOVE INSTRUMENT CLUSTER FINISH PANEL

9. REMOVE SPIRAL CABLE SUB-ASSEMBLY

10. REMOVE WIPER AND WASHER SWITCH ASSEMBLY

11. REMOVE HEADLIGHT DIMMER SWITCH ASSEMBLY

12. REMOVE INSTRUMENT PANEL SUB-ASSEMBLY UPPER

13. REMOVE INSTRUMENT PANEL SUB-ASSEMBLY LOWER

14. DISCONNECT STEERING SLIDING YOKE

15. DISCONNECT CONNECTOR

16. REMOVE STEERING COLUMN HOLE COVER SUB-ASSEMBLY

17. REMOVE STEERING COLUMN ASSEMBLY