GSIC - Global Service Information Center

# CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY > INSPECTION

## for Preparation Click here

1. INSPECT CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY

1. Measure the resistance between the terminals.

   Standard resistance:
     6.9 to 7.9 Ω at 20°C (68°F)
   If the result is not as specified, replace the oil control valve assembly.

1. Connect the battery's positive (+) lead to terminal 1 and negative (-) lead to terminal 2, and check the movement of the valve.

   Specified condition:

     Condition | Specified Condition
     Battery positive (+) voltage is applied | Valve moves in left arrow direction shown in the illustration
     Battery positive (+) voltage is cut off | Valve moves in right arrow direction shown in the illustration

   If the result is not as specified, replace the oil control valve assembly. If the valve cannot return properly because of foreign matter, a small pressure leak in the advanced direction may occur and a DTC may be output.