GSIC - Global Service Information Center

# FUEL TEMPERATURE SENSOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. DRAIN FUEL

3. REMOVE FUEL TEMPERATURE SENSOR

1. Disconnect the sensor connector.

1. Using a 19 mm deep socket wrench, remove the sensor.