GSIC - Global Service Information Center

# CLUTCH PEDAL (for RHD) > REASSEMBLY

## for Preparation Click here

1. INSTALL PEDAL SPRING HOOK (w/ Turn over)

1. Apply MP grease to the contact surface of the hook.

1. Install the hook.

2. INSTALL CLUTCH PEDAL TURN OVER BUSH (w/ Turn over)

1. Apply MP grease to the contact surface of the bush.

1. Install the bush.

3. INSTALL NO. 1 CLUTCH PEDAL CUSHION

1. Install the cushion to the clutch pedal.

4. INSTALL COLLAR

1. Apply MP grease to both sides of a collar and 2 new bushes.

1. Install the collar.

1. Install the 2 bushes.

5. INSTALL CLUTCH PEDAL SUB-ASSEMBLY

1. Install the clutch pedal to the clutch pedal support.

   Torque:
     37 N*m{ 377 kgf*cm , 27 ft.*lbf }

   HINT:
     Install the bolt from the left side of the vehicle.

1. w/ Turn over:
   Install the clutch pedal return spring.

6. INSTALL CLUTCH PEDAL SPRING HOLDER (w/ Turn over)

1. Apply MP grease to the contact surface of the clutch pedal spring holder.

1. Install the clutch pedal spring holder.

7. INSTALL CLUTCH PEDAL SPRING (w/ Turn over)

1. Install the spring.

1. Apply MP grease to the contact surface of the clutch pedal.