GSIC - Global Service Information Center

# FRONT SEAT OUTER BELT ASSEMBLY > INSPECTION

## for Preparation Click here

1. INSPECT FRONT SEAT OUTER BELT ASSY LH

NOTICE:

  Do not disassemble the retractor.

1. Before installing the seat belt, check the ELR.

   1. When the inclination of the retractor is 15° or less, check that the belt can be pulled from the retractor. When the inclination of the retractor is over 45°, check that the belt locks. If the operation is not as specified, replace the seat belt assembly.
      If the result is not as specified, replace the outer belt assembly.