GSIC - Global Service Information Center

# REAR DOOR BELT MOULDING > INSTALLATION

## for Preparation Click here

1. INSTALL REAR DOOR BELT MOULDING ASSEMBLY LH

1. Put protective tape on the upper part of the door.

1. Attach the claws to install the moulding.

   HINT:
     Confirm that the moulding is firmly installed.

2. INSTALL REAR DOOR TRIM BOARD SUB-ASSEMBLY LH

3. INSTALL REAR DOOR ARMREST BASE PANEL UPPER LH (w/ Power Window)

4. INSTALL DOOR PULL HANDLE

5. INSTALL REAR DOOR WINDOW REGULATOR HANDLE ASSEMBLY (w/o Power Window)

6. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

7. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.