GSIC - Global Service Information Center

# STARTER RELAY > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT STARTER RELAY

1. Remove the engine room relay block cover.

1. Remove the starter relay from the engine room relay block.

1. Measure the resistance of the starter relay.

   Standard resistance:

     Tester Connection | Specified Condition
     3 - 5 | 10 kΩ or higher
     3 - 5 | Below 1 Ω (when battery voltage is applied to terminals 1 and 2)

   If the result is not as specified, replace the relay.

1. Reinstall the starter relay to the engine room relay block.

1. Reinstall the engine room relay block cover.