GSIC - Global Service Information Center

# STARTER > INSTALLATION

## for Preparation Click here

1. INSTALL STARTER ASSEMBLY

1. Install the starter with the 2 bolts.

   Torque:
     37 N*m{ 377 kgf*cm , 27 ft.*lbf }

1. Install the starter wire to terminal 30 with the nut.

   Torque:
     9.8 N*m{ 100 kgf*cm , 87 in.*lbf }

1. Connect the starter connector.

1. Install the clutch release cylinder (Click here).

2. INSTALL FRONT FENDER SEAL

1. Install the fender seal with the 5 clips.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.