GSIC - Global Service Information Center

# CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY

1. Install a new O-ring to the oil control valve.

1. Install the oil control valve with the bolt.

   Torque:
     8.5 N*m{ 87 kgf*cm , 75 in.*lbf }

1. Connect the oil control valve connector.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.