GSIC - Global Service Information Center

# FRONT BUMPER > REASSEMBLY

## for Preparation Click here

1. INSTALL NO. 2 FRONT BUMPER EXTENSION INSERT LH

1. Install the extension insert with the screw.

2. INSTALL NO. 2 FRONT BUMPER EXTENSION INSERT RH

1. Install the extension insert with the screw.

3. INSTALL FRONT BUMPER HOLE COVER LH

1. Install the hole cover with the clip.

4. INSTALL FRONT BUMPER HOLE COVER RH

1. Install the hole cover with the clip.

5. INSTALL FRONT BUMPER EXTENSION LH (w/ Front Bumper Extension)

1. Install the extension with the 6 clips.

6. INSTALL FRONT BUMPER EXTENSION RH (w/ Front Bumper Extension)

HINT:

  Use the same procedures described for the LH side.

7. INSTALL RADIATOR GRILLE EMBLEM

1. Attach the 3 claws to install the emblem.

8. INSTALL RADIATOR GRILLE NAME PLATE (for 1GR-FE)

1. Clean the grille surface.

   1. Using a heat light, heat the grille surface.

      Standard:

        Item | Heating Temperature
        Radiator grille | 20 to 30°C (68 to 86°F)

      NOTICE:
        Do not heat the radiator grille excessively.

   2. Remove the double-sided tape from the grille.

   3. Wipe off any tape adhesive residue with cleaner.

1. Install a new name plate.

   1. Remove the peeling paper from the name plate.

   2. Install the name plate to the radiator grille.

   3. Securely attach 2 new spring nuts to the name plate.

9. INSTALL NO. 1 RADIATOR GRILLE RETAINER

1. Install the retainer with the 5 screws.