GSIC - Global Service Information Center

# LOWER INSTRUMENT PANEL > DISASSEMBLY

## for Preparation Click here

1. REMOVE NO. 1 SWITCH HOLE BASE

1. Detach the 4 claws and remove the switch hole base.

2. REMOVE FRONT ASH RECEPTACLE BOX SUB-ASSEMBLY

3. REMOVE FRONT ASH RECEPTACLE RETAINER SUB-ASSEMBLY

1. Remove the 2 screws <B> and retainer.

4. REMOVE INSTRUMENT PANEL BRACKET SUB-ASSEMBLY CENTER

1. Remove the screw <B> and bracket.

5. REMOVE NO. 1 INSTRUMENT PANEL MOUNTING BRACKET

1. Remove the screw <F> and bracket.