GSIC - Global Service Information Center

# INTERIOR > TORQUE SPECIFICATIONS

ROOF HEADLINING (DOUBLE CAB):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Front seat outer belt assembly (shoulder anchor) x Body | 42 | 428 | 31
  Front seat outer belt assembly (belt anchor) x Body | 42 | 428 | 31
  Rear No. 1 seat belt assembly outer (shoulder anchor) x Body | 42 | 428 | 31

ROOF HEADLINING (EXTRA CAB):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Front seat outer belt assembly (shoulder anchor) x Body | 42 | 428 | 31
  Front seat outer belt assembly (belt anchor) x Body | 42 | 428 | 31
  Rear No. 1 seat belt assembly outer (shoulder anchor) x Body | 42 | 428 | 31
  Rear No. 1 seat belt assembly outer (shoulder anchor) x Body | 42 | 428 | 31

ROOF HEADLINING (SINGLE CAB):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Front seat outer belt assembly (shoulder anchor) x Body | 42 | 428 | 31
  Front seat outer belt assembly (belt anchor) x Body | 42 | 428 | 31