GSIC - Global Service Information Center

# REAR SHOCK ABSORBER (for 4WD) > INSPECTION

## for Preparation Click here

1. INSPECT REAR SHOCK ABSORBER ASSEMBLY

1. Compress and extend the shock absorber rod, and check that there is no abnormal resistance or unusual sound during the operation.

   1. If there is any abnormality, replace the shock absorber with a new one.

      NOTICE:
        When disposing of the shock absorber, see DISPOSAL on page.