GSIC - Global Service Information Center

# PARKING BRAKE LEVER > INSTALLATION

## for Preparation Click here

1. INSTALL PARKING BRAKE LEVER SUB-ASSEMBLY

1. Install the switch to the lever with the screw.

1. Connect the switch connector.

1. Connect the cable to the lever with the 2 bolts and 2 nuts labeled A.

   Torque:
     14.5 N*m{ 148 kgf*cm , 11 ft.*lbf }

1. Return the claw labeled B to its original position.

1. Install the lever with the 2 nuts labeled C.

   Torque:
     12.5 N*m{ 127 kgf*cm , 9 ft.*lbf }

1. Install the wire adjusting nut and lock nut labeled D.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

2. CHECK PARKING BRAKE LEVER TRAVEL

1. Pull the lever upward with a force of approximately 200 N (20 kgf, 44 lbf) and count the number of clicks.

   OK:
     7 to 9 clicks

3. ADJUST PARKING BRAKE LEVER TRAVEL

1. Remove the lock nut.

1. Turn the No. 1 wire adjusting nut until the lever travel is correct.

1. Tighten the lock nut.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

   HINT:
     If further adjustment is necessary, proceed to the next step.

4. ADJUST PARKING BRAKE TURN BUCKLE

1. Loosen the lock nut and turn the buckle until the lever travel is correct.

1. Tighten the lock nut.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

5. INSTALL CONSOLE BOX ASSEMBLY

1. Install the console box with the 2 clips, 4 screws <F> and 2 bolts <E>.

6. INSTALL CONSOLE PANEL SUB-ASSEMBLY

NOTICE:

  Be careful not to damage the instrument panel lower and console box with the claws of the console panel upper.

1. Attach the 12 claws to install the console panel.

7. INSTALL PARKING BRAKE HOLE COVER SUB-ASSEMBLY

1. Attach the 4 claws to install the hole cover.

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.