GSIC - Global Service Information Center

# FRONT SHOCK ABSORBER WITH COIL SPRING (for 4WD) > DISPOSAL

## for Preparation Click here

1. DISPOSE OF FRONT SHOCK ABSORBER ASSEMBLY

1. Fully extend the shock absorber piston rod, and clamp it in a vise at an angle.

1. Using a drill or similar tool, gradually make a hole in area A to discharge the gas inside of the absorber.

   CAUTION:
     As metal debris may be blown outward by the gas, you must:
   1. Wear protective glasses.
   1. Cover the area being cut.

   NOTICE:
     The gas is colorless and harmless.