GSIC - Global Service Information Center

# COMPRESSOR AND PULLEY (for 2KD-FTV) > INSPECTION

## for Preparation Click here

1. INSPECT COOLER COMPRESSOR ASSEMBLY

1. Check the operation.

   1. Start the engine.

   2. Inspect the compressor pulley.

      OK:
        Compressor shaft rotates along with pulley.

1. Inspect the cooler compressor.

   1. Disconnect the connector.

   2. Apply battery voltage to the clutch and check operation of the clutch.

      OK:

        Measurement Condition | Specified Condition
        Battery positive (+) → Terminal 1 Battery negative (-) → Body ground | Magnet clutch is engaged

      If the result is not as specified, replace the compressor.