GSIC - Global Service Information Center

# INTAKE AIR TEMPERATURE SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL INTAKE AIR TEMPERATURE SENSOR

1. Using a 22 mm deep socket wrench, install a new gasket and the IAT sensor.

   Torque:
     29 N*m{ 296 kgf*cm , 21 ft.*lbf }

1. Connect the IAT sensor connector.

2. INSTALL ENGINE COVER SUB-ASSEMBLY

1. Install the cover with the 3 bolts and 2 nuts.

   Torque:
     7.0 N*m{ 71 kgf*cm , 62 in.*lbf }

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.