GSIC - Global Service Information Center

# HORN SYSTEM > INSPECTION

## for Preparation Click here

1. INSPECT FUSE (HORN)

1. Measure the resistance of the HORN fuse.

   Standard resistance:
     Below 1 Ω
   If the result is not as specified, replace the fuse.

2. INSPECT HORN ASSEMBLY

1. Apply battery voltage and check operation of the horn.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → Terminal 1 Battery negative (-) → Horn bracket | Horn sounds

   If the result is not as specified, replace the horn assembly.