GSIC - Global Service Information Center

# FRONT AIRBAG SENSOR > INSTALLATION

## for Preparation Click here

CAUTION:

  Be sure to read the precautionary notices concerning the SRS airbag system before servicing (Click here).

1. INSTALL FRONT AIRBAG SENSOR LH

1. Install the sensor with the nut.

   Torque:
     17.5 N*m{ 179 kgf*cm , 13 ft.*lbf }

   NOTICE:
   1. If the airbag sensor has been dropped, or there are any cracks, dents or other defects in the case or connector, replace it with a new one.
   2. When installing the airbag sensor, make sure that the SRS wiring does not interfere with other parts and is not pinched between other parts.

1. Check that there is no free play in the installation parts of the sensor.

1. Connect the sensor connector.

2. INSTALL FRONT AIRBAG SENSOR RH

1. Install the sensor with the nut.

   Torque:
     17.5 N*m{ 179 kgf*cm , 13 ft.*lbf }

   NOTICE:
   1. If the airbag sensor has been dropped, or there are any cracks, dents or other defects in the case or connector, replace it with a new one.
   2. When installing the airbag sensor, make sure that the SRS wiring does not interfere with other parts and is not pinched between other parts.

1. Check that there is no free play in the installation parts of the sensor.

1. Connect the sensor connector.

3. INSTALL BATTERY (LH SIDE)

1. Install the battery.

1. Install the battery stay with the 2 bolts.

1. Connect the cable to the positive (+) battery terminal.

4. INSTALL AIR CLEANER ASSEMBLY (RH SIDE)

1. (1TR-FE: see page , 2TR-FE: see page , 1GR-FE: see page , 1KD-FTV: see page , 2KD-FTV: see page )

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. INSTALL RADIATOR GRILLE

1. Push the radiator grille in the direction indicated by the arrow in the illustration. Attach the 5 claws to install the radiator grille.

1. Install the 2 screws and 2 clips.

7. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

8. INSPECT SRS WARNING LIGHT

1. Check the SRS warning light (Click here).