GSIC - Global Service Information Center

# MANUAL TRANSMISSION OIL > ON-VEHICLE INSPECTION

## for Preparation Click here

1. CHECK TRANSMISSION OIL

1. Stop the vehicle on a level surface.

1. Remove the filler plug and gasket.

1. Check that the oil level is between 0 to 5 mm (0 to 0.20 in.) from the bottom lip of the filler plug opening.
   If the result is not as specified, add transmission oil.

   Oil grade:
     GL-4 or GL-5

   Viscosity:
     SAE 75W-90

   Capacity:
     2.2 liters (2.3 US qts, 1.9 lmp. qts)

   NOTICE:
   1. Too much or too little oil will lead to transmission problems.
   2. After adjusting the oil level, drive the vehicle and check the oil level again.

1. Check for oil leakage when the oil level is low. If leakage is found, repair the area necessary to stop the leak. Replace damaged parts as necessary.

1. Install a new gasket and the filler plug.

   Torque:
     37 N*m (377 kgf*cm, 27 ft.*lbf)