GSIC - Global Service Information Center

# ELECTRONIC CONTROLLED AUTOMATIC TRANSMISSION SYSTEM > PRECAUTION

## for Preparation Click here

NOTICE:

1. When disconnecting the cable from the negative (-) battery terminal, initialize the following system(s) after the cable is reconnected.

   System Name | See procedure
   Combination meter | Click here

2. Perform the RESET MEMORY procedure (A/T initialization) when replacing the automatic transmission assembly, engine assembly or ECM (Click here).

HINT:

  RESET MEMORY cannot be completed by only reconnecting the cable to the negative (-) battery terminal.