GSIC - Global Service Information Center

# STOP LIGHT SWITCH > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE STOP LIGHT SWITCH ASSEMBLY

1. Turn the switch counterclockwise and remove it.

1. Remove the adjuster from the support.