GSIC - Global Service Information Center

# CLUTCH > SERVICE DATA

Pedal height from dash panel | 179.6 to 189.6 mm (7.070 to 7.464 in.)
Clutch pedal free play | 5.0 to 15.0 mm (0.197 to 0.591 in.)
Clutch pedal push rod play at pedal top | 1.0 to 5.0 mm (0.039 to 0.197 in.)
Disc rivet head depth | Minimum. | 0.3 mm (0.012 in.)
Disc runout | Minimum. | 0.8 mm (0.031 in.)
Diaghargm spring finger wear | Maximum. depth | 0.5 mm (0.020 in.)
Maximum. width | 6.0 mm (0.236 in.)
Flywheel runout | Maximum. | 0.1 mm (0.004 in.)
Diaghargm spring finger wear | Maximum. depth | 0.5 mm (0.020 in.)
Clutch release point from pedal full stroke end position | 25 mm (0.98 in.) or more