GSIC - Global Service Information Center

# REAR PLANETARY GEAR > INSPECTION

## for Preparation Click here

1. INSPECT NO. 2 ONE-WAY CLUTCH

1. Hold the planetary gear and turn the one-way clutch inner race. Check that the one-way clutch inner race can be turned freely counterclockwise and locks when turned clockwise.

2. INSPECT PLANETARY PINION GEAR THRUST CLEARANCE

1. Using a feeler gauge, measure the thrust clearance.

   Standard clearance:
     0.20 to 0.60 mm (0.0079 to 0.0236 in.)

   Maximum clearance:
     0.65 mm (0.0256 in.)
   If the clearance is greater than the maximum, replace the planetary gear.

3. INSPECT NO. 2 ONE-WAY CLUTCH

1. Hold the planetary gear and turn the one-way clutch inner race. Check that the one-way clutch inner race can be turned freely counterclockwise and locks when turned clockwise.