GSIC - Global Service Information Center

# REAR AXLE SHAFT > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH side.
2. The procedures listed below are for the LH side.
3. A bolt without a torque specification is shown in the standard bolt chart (Click here).

1. INSTALL REAR AXLE SHAFT BEARING

1. Using SST and a press, press in a new bearing.

   SST
     09515-30010
     09950-60020 (09951-00890)

2. INSTALL REAR AXLE SHAFT OUTER OIL SEAL

1. Using SST and a hammer, tap in a new oil seal.

   SST
     09950-60010 (09951-00610)
     09950-70010 (09951-07150)

3. INSTALL REAR AXLE HUB BOLT

1. Install a new deflector gasket and the deflector to the axle shaft.

   HINT:
     Align the 2 notches.

1. Pass the bolts through the axle hub.

1. Temporarily install a plate washer and nut to the bolt. Install the hub bolt by tightening the nut.

1. Remove the nut and plate washer.

4. INSTALL BACKING PLATE

1. Position the backing plate on the bearing case.

1. Using 2 socket wrenches, press in the serration bolts.

5. INSTALL REAR AXLE SHAFT IN BACKING PLATE

1. Coat a new oil seal lip with MP grease.

1. Install the backing plate and bearing retainer on the rear axle shaft.

1. Using SST and a press, press in the axle shaft into the backing plate.

   SST
     09316-60011 (09316-00051)

1. Using snap ring expander, install a new snap ring.

6. INSTALL REAR AXLE BEARING RETAINER AND ABS SPEED SENSOR ROTOR (w/ ABS)

1. Using SST and a press, press in a new sensor rotor and new bearing retainer to the axle shaft until length is within the standard range.

   SST
     09316-60011 (09316-00051)

   Standard length:
     12.2 +- 0.6 mm (4.811 +- 0.024 in.)

   NOTICE:
     Oil leakage may occur if length is not within the standard range and the lip of the oil seal does not contact to the retainer.

7. REMOVE REAR AXLE SHAFT OIL SEAL

1. Using SST and a hammer, tap in a new oil seal.

   SST
     09950-60020 (09951-00770)
     09950-70010 (09951-07150)

1. Coat the lip of the oil seal with MP grease.

8. INSTALL REAR AXLE SHAFT WITH BACKING PLATE

1. Install a new O-ring.

1. Install the axle shaft with the 4 nuts.

   Torque:
     69 N*m{ 704 kgf*cm , 51 ft.*lbf }

9. INSTALL BRAKE LINE AND PARKING BRAKE CABLE

1. Using SST, connect the brake tube.

   SST
     09023-00101

   Torque:
     15 N*m{ 155 kgf*cm , 11 ft.*lbf }
     14 N*m{ 143 kgf*cm , 10 ft.*lbf } for use with SST

   HINT:
     Use a torque wrench with a fulcrum length of 30 cm (11.81 in.).

1. Connect the parking brake cable with the 2 bolts.

10. INSTALL REAR BRAKE SHOE (for 2WD)

1. Install the rear brake shoe (Click here).

11. INSTALL REAR BRAKE SHOE (for 4WD)

1. Install the rear brake shoe (Click here).

12. INSTALL BRAKE DRUM

13. INSTALL SPEED SENSOR REAR LH (w/ ABS)

1. Install the sensor with the bolt.

   Torque:
     8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

   NOTICE:
     Make sure the sensor tip is clean.

1. Connect the sensor connector.

14. BLEED AIR FROM BRAKE LINE

1. Bleed air from the brake line (Click here).

15. CHECK BRAKE FLUID LEVEL IN RESERVOIR

1. Check the brake fluid level in the reservoir (Click here).

16. CHECK FOR BRAKE FLUID LEAKAGE

17. INSTALL REAR WHEEL

Torque:
  152 N*m{ 1,550 kgf*cm , 112 ft.*lbf } for 2WD (steel type)
  121 N*m{ 1,234 kgf*cm , 89 ft.*lbf } for 2WD (aluminum type)
  105 N*m{ 1,071 kgf*cm , 77 ft.*lbf } for 4WD

18. INSPECT AND ADJUST PARKING BRAKE LEVER TRAVEL

1. Inspect and adjust parking brake lever travel (Click here).

19. CHECK ABS SPEED SENSOR SIGNAL (w/ ABS)

1. Check ABS speed sensor signal (Click here).