GSIC - Global Service Information Center

# HEADLIGHT ASSEMBLY > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH side.
2. The procedures listed below are for the LH side.
3. A bolt without a torque specification is shown in the standard bolt chart (see page @@-@@@)

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE RADIATOR GRILLE

1. Using a clip remover, remove the 2 clips.

1. Remove the 2 screws.

1. Pull the radiator grille in the direction indicated by the arrow in the illustration to detach the 5 claws and remove the radiator grille.

3. REMOVE FRONT FENDER LINER LH

1. Remove the screw.

1. Using a clip remover, remove the 3 clips.

1. Partially remove the fender liner.

   HINT:
     It is not necessary to fully remove the fender liner. Partially remove it so that the bumper cover can be removed in a later step.

4. REMOVE ENGINE SIDE COVER SUB-ASSEMBLY LH (for 4WD)

1. Using a clip remover, remove the 2 clips.

1. Remove the 3 bolts and engine side cover.

5. REMOVE ENGINE SIDE COVER SUB-ASSEMBLY RH (for 4WD)

HINT:

  Use the same procedures described for the LH side.

6. REMOVE FRONT BUMPER COVER

1. Using a clip remover, remove the 9 clips.

1. Put protective tape under the front fender.

1. Detach the 4 claws and remove the bumper cover.

7. REMOVE HEADLIGHT ASSEMBLY

1. Remove the 3 screws and bolt.

1. Disconnect the connectors and remove the headlight.

8. REMOVE HEADLIGHT SOCKET COVER

9. REMOVE NO. 1 HEADLIGHT BULB

1. Release the lock of the set spring and remove the bulb.

10. REMOVE FRONT TURN SIGNAL LIGHT BULB

1. Turn the bulb/socket unit in the direction indicated by the arrow and pull to remove it.

1. Remove the bulb from the socket.

11. REMOVE CLEARANCE LIGHT BULB

1. Turn the bulb in the direction indicated by the arrow and pull to remove it.