GSIC - Global Service Information Center

# REAR SEAT ASSEMBLY (for Extra Cab) > REMOVAL

## for Preparation Click here

1. REMOVE REAR SEAT CUSHION ASSEMBLY LH

1. Pull the seat cushion lock hook's release lever in the direction of the arrow, and then disconnect the hook on the front of the seat cushion.

1. Detach the seat cushion's 2 rear hooks from the vehicle body.

1. Remove the seat cushion.

2. REMOVE REAR SEAT CUSHION ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.

3. REMOVE BACK PANEL GARNISH UPPER

1. Using a screwdriver, detach the 4 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

4. REMOVE BACK PANEL GARNISH LOWER

1. Using a screwdriver, detach the 6 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

5. REMOVE REAR SEATBACK ASSEMBLY

1. Remove the 2 bolts.

1. Lift up the seatback in the direction indicated by the arrow in the illustration to detach the 2 hooks from the vehicle body. Then remove the seatback.

   NOTICE:
     Be careful not to damage the vehicle body.