GSIC - Global Service Information Center

### REAR SPEAKER (for Extra Cab) > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE BACK PANEL GARNISH UPPER

3. REMOVE REAR SEAT CUSHION ASSEMBLY LH

4. REMOVE REAR SEAT CUSHION ASSEMBLY RH

5. REMOVE BACK PANEL GARNISH LOWER

6. REMOVE REAR SEATBACK ASSEMBLY

7. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

8. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

9. REMOVE QUARTER INSIDE TRIM BOARD

10. REMOVE REAR NO. 1 SPEAKER ASSEMBLY