GSIC - Global Service Information Center

# FRONT DOOR COURTESY SWITCH > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH sides.
2. The procedures listed below are for the LH side.
3. A bolt without a torque specification is shown in the standard bolt chart (Click here).

1. INSTALL FRONT DOOR COURTESY LIGHT SWITCH ASSEMBLY

1. Connect the connector.

1. Install the bolt and switch.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.