GSIC - Global Service Information Center

# FRONT PROPELLER SHAFT ASSEMBLY > REASSEMBLY

## for Preparation Click here

1. INSTALL UNIVERSAL JOINT SPIDER ASSEMBLY

1. Apply MP grease to a new spider and 2 new spider bearings.

1. Fit the spider into the flange yoke.

1. Using SST, install the 2 spider bearings to the spider.

   SST
     09332-25010

1. Using SST, adjust the spider bearings so that: 1) the flange yoke does not overlap the snap ring grooves of the spider bearings, and the grooves are as wide as possible; and 2) the groove width on both sides is the same.

   SST
     09332-25010

1. Install 2 new snap rings to the installed spider bearings. The snap rings must have equal thickness which will allow 0 to 0.05 mm (0 to o.0020 in.) of axial play.

   Thickness of snap ring:

     Part No. | Thickness | Mark
     90520-T0007 | 2.19 mm (0.0862 in.) | F
     90520-T0008 | 2.21 mm (0.0870 in.) | G
     90520-T0009 | 2.23 mm (0.0877 in.) | H
     90520-T0010 | 2.25 mm (0.0885 in.) | J
     90520-T0011 | 2.27 mm (0.0893 in.) | K
     90520-T0012 | 2.29 mm (0.0901 in.) | 1
     90520-T0013 | 2.31 mm (0.0909 in.) | 2
     90520-T0014 | 2.33 mm (0.0917 in.) | 3
     90520-T0015 | 2.35 mm (0.0925 in.) | 4
     90520-T0016 | 2.37 mm (0.0933 in.) | 5
     90520-T0017 | 2.39 mm (0.0940 in.) | 6
     90520-T0018 | 2.41 mm (0.0948 in.) | 7
     90520-T0019 | 2.43 mm (0.0956 in.) | 8
     90520-T0020 | 2.45 mm (0.0964 in.) | N
     90520-T0021 | 2.47 mm (0.0972 in.) | 10
     90520-T0022 | 2.49 mm (0.0980 in.) | A
     90520-T0023 | 2.51 mm (0.0988 in.) | B
     90520-T0024 | 2.53 mm (0.0996 in.) | C
     90520-T0025 | 2.55 mm (0.1003 in.) | D
     90520-T0026 | 2.57 mm (0.1011 in.) | E

   NOTICE:
   1. New snap rings must be used.
   2. The snap ring thickness must be the same on both ends.

1. Using a hammer, tap the flange yoke until there is no clearance between the spider bearings and snap rings.

1. Align the matchmarks on the flange yoke and sleeve yoke.

1. Install new spider bearings on the sleeve yoke side.

   HINT:
     Use the procedures described above.

2. INSPECT UNIVERSAL JOINT SPIDER ASSEMBLY

1. Check the spider bearings for wear or damage.

1. Check each spider bearing's axial play by turning the yoke while holding the shaft tightly.

   Maximum bearing axial play:
     0.05 mm (0.0020 in.)
   If the bearing axial play is greater than the maximum, replace the spider bearing.

3. INSPECT PROPELLER SHAFT GREASE FITTING DIRECTION

HINT:

  When replacing a spider bearing, be sure that the grease fitting hole is facing the direction shown in the illustration.