GSIC - Global Service Information Center

# BACK-UP LIGHT SWITCH > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE BACK-UP LIGHT SWITCH ASSEMBLY

1. Using SST, remove the back-up light switch and gasket from the transmission case.

   SST
     09817-16011