GSIC - Global Service Information Center

# HEATED OXYGEN SENSOR (for Sensor 2) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE HEATED OXYGEN SENSOR (for Bank 1 Sensor 2)

1. Disconnect the sensor connector.

1. Using SST, remove the sensor from the front exhaust pipe.

   SST
     09224-00010

3. REMOVE HEATED OXYGEN SENSOR (for Bank 2 Sensor 2)

1. Disconnect the sensor connector.

1. Using SST, remove the sensor from the front exhaust pipe.

   SST
     09224-00010