GSIC - Global Service Information Center

# HAZARD WARNING SWITCH > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH sides.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE INSTRUMENT CLUSTER FINISH PANEL ASSEMBLY CENTER

HINT:

  To prevent the clips from falling, horizontally pull out the panel. Hold both sides of the panel in the locations indicated by the arrows in the illustration.

1. Remove the screw <C>.

1. Detach the 6 claws and 4 clips.

1. NOTICE:
     Make sure the center registers are not removed.
   Disconnect all connectors and remove the panel.

3. REMOVE HEATER CONTROL KNOB

1. Remove the 3 control knobs.

4. REMOVE FRE/REC CONTROL KNOB

1. Remove the control knob.

5. REMOVE HAZARD WARNING SIGNAL SWITCH ASSEMBLY

1. Detach the 2 claws and remove the switch.