GSIC - Global Service Information Center

### AIR PUMP (for Unleaded Gasoline Specification Vehicle) > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE AIR CLEANER ASSEMBLY

3. REMOVE AIR PUMP INLET

4. DISCONNECT NO. 4 AIR HOSE

5. REMOVE AIR PUMP PIPE

6. REMOVE FRONT FENDER APRON SEAL UPPER

7. REMOVE AIR PUMP ASSEMBLY WITH BRACKET

8. REMOVE AIR PUMP COVER

9. DISCONNECT NO. 2 AIR HOSE

10. DISCONNECT NO. 3 AIR HOSE

11. REMOVE AIR PUMP ASSEMBLY